[GENERAL]
Rules=0
GarageDisplayFlags=7
FeelerFlags=0
Mass=1240
Inertia=(1325.491,1722.449,397.131)
FuelTankPos=(0.00, 0.14, -0.40)
FuelTankMotion=(560.0,0.7)
Notes="288gto"
Symmetric=1
DamageFile=288GTO_damage
CGHeight=0.292
CGRightRange=(0.500, 0.005, 1)
CGRightSetting=0
CGRearRange=(0.54, 0.000, 1)
CGRearSetting=0
GraphicalOffset=(0.0, -0.105, 0.0)
Undertray00=( 0.83, 0.0, -2.05) // corner offset from center of vehicle
Undertray01=(-0.83, 0.0, -2.05)
Undertray02=( 0.95, 0.0,  1.035)
Undertray03=(-0.95, 0.0,  1.035)
Undertray04=( 0.00, 0.00, -2.25)
Undertray05=( 0.78, 0.1,  2.15)
Undertray06=(-0.78, 0.1,  2.15)
Undertray07=( 0.00, 0.00, 2.25)
UndertrayParams=(320000.0,12000.0,3.5) // spring/damper/friction
TireBrand=288stradale_tires
FrontTireCompoundSetting=0
RearTireCompoundSetting=0
FuelRange=(1.0, 1.0, 100)
FuelSetting=25
NumPitstopsRange=(0, 1, 4)
NumPitstopsSetting=3
Pitstop1Range=(1.0, 1.0, 100)
Pitstop1Setting=25
Pitstop2Range=(1.0, 1.0, 100)
Pitstop2Setting=25
Pitstop3Range=(1.0, 1.0, 100)
Pitstop3Setting=25
AIAimSpeedsPerWP=(25.0, 35.0, 45.0, 55.0, 65.0, 75.0, 85.0, 95.0, 105.0, 115.0, 125.0)
AICornerReductionBase=70.0
AIMinPassesPerTick=3
AIRotationThreshold=0.70
AIEvenSuspension=1.0
AISpringRate=1.0
AIDamperSlow=0.8
AIDamperFast=0.3
AIDownforceZArm=0.0
AIDownforceBias=0.0
AITorqueStab=(0.72, 0.8, 0.8)

[BODYAERO]
BodyDragBase=(0.368)            // base drag
BodyDragHeightAvg=(0.01)       // drag increase with average ride height
BodyDragHeightDiff=(0.02)       // drag increase with front/rear ride height difference
BodyMaxHeight=(0.00)            // maximum ride height that affects drag/lift
BodyLeft=(-0.85, 0.0, 0.0)       // aero forces from moving left
BodyRight=(0.85, 0.0, 0.0)       // aero forces from moving right
BodyUp=(0.0, -1.5, 0.0)         // aero forces from moving up
BodyDown=(0.0, 1.5, 0.0)        // aero forces from moving down
BodyAft=(0.0, 0.10, -1.00)      // aero forces from moving rearwards
BodyFore=(0.0, -0.275, 0.200)   // aero forces from moving forwards (lift value important, but drag overwritten)
BodyRot=(3.0, 2.0, 1.5)         // aero torque from rotating
BodyCenter=(0.0, 0.450, -1.067) // center of body aero forces (offset from center of rear axle at ref plane)
RadiatorRange=(100.0, -5.0, 1)  // radiator range (front grille tape)
RadiatorSetting=0               // radiator setting
RadiatorDrag=(0.00)              // effect of radiator setting on drag
RadiatorLift=(0.00)              // effect of radiator setting on lift
BrakeDuctRange=(0.0, 1.0, 1)    // brake duct range
BrakeDuctSetting=0              // brake duct setting
BrakeDuctDrag=(0.0)             // effect of brake duct setting on drag
BrakeDuctLift=(0.000)             // effect of brake duct setting on lift


[SUSPENSION]
PhysicalModelFile=288GTO_stradale.pm
CorrectedInnerSuspHeight=-1
ApplySlowToFastDampers=0
AdjustSuspRates=0
AlignWheels=1
FrontWheelTrack=1.56
RearWheelTrack=0.0
LeftWheelBase=2.45
RightWheelBase=2.45
SpringBasedAntiSway=1
AllowNoAntiSway=0
FrontAntiSwayBase=0
FrontAntiSwayRange=(0,1000,40)
FrontAntiSwaySetting=25
RearAntiSwayBase=0
RearAntiSwayRange=(0,1000,20)
RearAntiSwaySetting=5
LeftCasterRange=(5,0.1,1)
LeftCasterSetting=0
RightCasterRange=(5,0.1,1)
RightCasterSetting=0
FrontToeInRange=(-0.1, 0.1, 0)
FrontToeInSetting=0
RearToeInRange=(0.1, 0.1, 0)
RearToeInSetting=0

[CONTROLS]
SteeringFFBMult=5.0
SteerLockRange=(5.0, 0.5, 57)
SteerLockSetting=30
RearBrakeRange=(0.390,0.01,50)
RearBrakeSetting=0
BrakePressureRange=(0.80, 0.01, 21)
BrakePressureSetting=20
HandbrakePressRange=(0.01, 0.01, 120)
HandbrakePressSetting=89
AutoUpshiftGripThresh=0.63
AutoDownshiftGripThresh=0.63
TractionControlGrip=(1.00, 0.20)
TractionControlLevel=(0.30, 0.90)
ABS4Wheel=1
ABSGrip=(1.00, 0.20)
ABSLevel=(0.30, 0.90)
OnboardBrakeBias=0


[ENGINE]
SpeedLimiter=0
Normal=288GTO_engine.ini
RestrictorPlate=288GTO_engine.ini

[DRIVELINE]
ClutchInertia=0.0300
ClutchTorque=1500.0
ClutchWear=0.0
ClutchFriction=17.00
ClutchEngageRate=2.2
BaulkTorque=500.0
AllowManualOverride=0
SemiAutomatic=0
UpshiftDelay=0.42
UpshiftClutchTime=0.27
DownshiftDelay=0.42
DownshiftClutchTime=0.27
DownshiftBlipThrottle=0.70
WheelDrive=REAR
GearFile=288GTO_Gears.ini
AllowGearingChanges=0
AllowFinalDriveChanges=0
FinalDriveSetting=0
ReverseSetting=0
ForwardGears=5
Gear1Setting=1
Gear2Setting=2
Gear3Setting=3
Gear4Setting=4
Gear5Setting=5
DiffPumpTorque=150.0                // at 100% pump diff setting, the torque redirected per wheelspeed difference in radians/sec (roughly 1.2kph)
DiffPumpRange=(0.50,0,1)          // differential acting on all driven wheels
DiffPumpSetting=0
DiffPowerRange=(0.2,0,1)         // fraction of power-side input torque transferred through diff
DiffPowerSetting=1                  // (not implemented for four-wheel drive)
DiffCoastRange=(0.4,0,1)       // fraction of coast-side input torque transferred through diff
DiffCoastSetting=1  
DiffPreloadRange=(0,0,1)     // preload torque that must be overcome to have wheelspeed difference
DiffPreloadSetting=0 

[FRONTLEFT]
BumpTravel=-0.05
ReboundTravel=-0.15
BumpStopSpring=200000
BumpStopRisingSpring=15000000
BumpStopDamper=2000
BumpStopRisingDamper=1000000
BumpStage2=0.175
ReboundStage2=-0.175
FrictionTorque=6
SpinInertia=1.6
CGOffsetX=0
PushrodSpindle=(0,0,0)
PushrodBody=(-0.1772,0.38,0)
CamberRange=(-2.3,0.1,40)
CamberSetting=10
PressureRange=(80,1,201)
PressureSetting=100
SpringMult=0.64
SpringRange=(33658.02,0,1)
SpringSetting=0
RideHeightRange=(0.1,0,1)
RideHeightSetting=0
DamperMult=1.21744
BumpStage2=0.15
ReboundStage2=-0.15
SlowBumpRange=(2018.94661,0,1)
SlowBumpSetting=0
FastBumpRange=(1009.47331,0,1)
FastBumpSetting=0
SlowReboundRange=(4542.62988,0,1)
SlowReboundSetting=0
FastReboundRange=(2271.31494,0,1)
FastReboundSetting=0
BrakeDiscRange=(0.038, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.45
BrakeOptimumTemp=500
BrakeFadeRange=850
BrakeWearRate=0.00000000001215
BrakeFailure=(1.33e-002,7.20e-004)
BrakeTorque=2600
BrakeHeating=0.00047
BrakeCooling=(1.720e-002,0.600e-004)
BrakeDuctCooling=0.00018

[FRONTRIGHT]
BumpTravel=-0.05
ReboundTravel=-0.15
BumpStopSpring=200000
BumpStopRisingSpring=15000000
BumpStopDamper=2000
BumpStopRisingDamper=1000000
BumpStage2=0.175
ReboundStage2=-0.175
FrictionTorque=6
SpinInertia=1.6
CGOffsetX=0
PushrodSpindle=(0,0,0)
PushrodBody=(-0.1772,0.38,0)
CamberRange=(-2.3,0.1,40)
CamberSetting=10
PressureRange=(80,1,201)
PressureSetting=100
SpringMult=0.64
SpringRange=(33658.02,0,1)
SpringSetting=0
RideHeightRange=(0.1,0,1)
RideHeightSetting=0
DamperMult=1.21744
BumpStage2=0.15
ReboundStage2=-0.15
SlowBumpRange=(2018.94661,0,1)
SlowBumpSetting=0
FastBumpRange=(1009.47331,0,1)
FastBumpSetting=0
SlowReboundRange=(4542.62988,0,1)
SlowReboundSetting=0
FastReboundRange=(2271.31494,0,1)
FastReboundSetting=0
BrakeDiscRange=(0.038, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.45
BrakeOptimumTemp=500
BrakeFadeRange=850
BrakeWearRate=0.00000000001215
BrakeFailure=(1.33e-002,7.20e-004)
BrakeTorque=2600
BrakeHeating=0.00047
BrakeCooling=(1.720e-002,0.600e-004)
BrakeDuctCooling=0.00018

[REARLEFT]
BumpTravel=-0.06
ReboundTravel=-0.16
BumpStopSpring=200000
BumpStopRisingSpring=15000000
BumpStopDamper=2000
BumpStopRisingDamper=1000000
BumpStage2=0.175
ReboundStage2=-0.175
FrictionTorque=6
SpinInertia=1.8
CGOffsetX=0
PushrodSpindle=(0,0,0)
PushrodBody=(-0.17778,0.38125,0)
CamberRange=(-2.3,0.1,40)
CamberSetting=10
PressureRange=(80,1,201)
PressureSetting=100
SpringMult=0.59172
SpringRange=(53760.80295,0,1)
SpringSetting=0
RideHeightRange=(0.11,0,1)
RideHeightSetting=0
DamperMult=1.21744
BumpStage2=0.15
ReboundStage2=-0.15
SlowBumpRange=(2643.53712,0,1)
SlowBumpSetting=0
FastBumpRange=(1321.76856,0,1)
FastBumpSetting=0
SlowReboundRange=(5947.95852,0,1)
SlowReboundSetting=0
FastReboundRange=(2973.97926,0,1)
FastReboundSetting=0
BrakeDiscRange=(0.0355, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.35
BrakeOptimumTemp=500
BrakeFadeRange=850
BrakeWearRate=0.00000000001215
BrakeFailure=(1.33e-002,7.20e-004)
BrakeTorque=2100
BrakeHeating=0.00045
BrakeCooling=(1.720e-002,0.600e-004)
BrakeDuctCooling=0.00018

[REARRIGHT]
BumpTravel=-0.06
ReboundTravel=-0.16
BumpStopSpring=200000
BumpStopRisingSpring=15000000
BumpStopDamper=2000
BumpStopRisingDamper=1000000
BumpStage2=0.175
ReboundStage2=-0.175
FrictionTorque=6
SpinInertia=1.8
CGOffsetX=0
PushrodSpindle=(0,0,0)
PushrodBody=(0.17778,0.38125,0)
CamberRange=(-2.3,0.1,40)
CamberSetting=10
PressureRange=(80,1,201)
PressureSetting=100
SpringMult=0.59172
SpringRange=(53760.80295,0,1)
SpringSetting=0
RideHeightRange=(0.11,0,1)
RideHeightSetting=0
DamperMult=1.21744
BumpStage2=0.15
ReboundStage2=-0.15
SlowBumpRange=(2643.53712,0,1)
SlowBumpSetting=0
FastBumpRange=(1321.76856,0,1)
FastBumpSetting=0
SlowReboundRange=(5947.95852,0,1)
SlowReboundSetting=0
FastReboundRange=(2973.97926,0,1)
FastReboundSetting=0
BrakeDiscRange=(0.0355, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.35
BrakeOptimumTemp=500
BrakeFadeRange=850
BrakeWearRate=0.00000000001215
BrakeFailure=(1.33e-002,7.20e-004)
BrakeTorque=2100
BrakeHeating=0.00045
BrakeCooling=(1.720e-002,0.600e-004)
BrakeDuctCooling=0.00018
